English.

This is a restoration utility for Asus WL500gP v1 & RT-N16.

How to:
1º Uncompress and install Restoration software in your PC.
2º Set up a manual IP in your network card (i.e: 192.168.1.5 , mask 255.255.255.0, gateway 192.168.1.1)
3º Coonect an ethernet cable between your network card and any of LAN RJ45 router sockets.
4º Disable any firewall or security block program in your PC.
5º Launch Firmware Restoration utilty in Asus utility program group (Important, if you run Windows 7 launch as administrator).
6º With your router unplugged from power supply press reset button and then connect power supply to the router.
7º Power LED should blink at 1 second on7off cicle. Release reset.
8º In the restoration utility GUI select wl500g-clearnvram.trx file and install, wait for 3 minutes and unplug router power supply.
9º With your router unplugged from power supply press reset button and then connect power supply to the router.
10º Power LED should blink at 1 second on7off cicle. Release reset.
11º In the restoration utility GUI select wl500g-recover.trx file and install, wait for 3 minutes and unplug router power supply.
9º With your router unplugged from power supply press reset button and then connect power supply to the router.
10º Power LED should blink at 1 second on7off cicle. Release reset.
11º In the restoration utility GUI select the apropiate firmware version for your router model and install, wait for 3 minutes and unplug router power supply.
12º Set up automatic settings for your network card.
13º Plug your router
14º You can access your router GUI again by entering 192.168.1.1 in your Internet browser, user = admin , password = admin in case of dd-wrt fix your login and credentials in the welcome screen.... but remember what you typed later.

-----------------------------
Notes: 
If you want to upgrade to dd-wrt install dd-wrt.v24-13491_NEWD_mini_asus.trx in step 11.
If you want to upgarde to Tomato RAF firmware in the router GUI (Inetrnet Browser) selecting firmware upgrade after dd-wrt has been installed.

Español.

¿Como instalar un nuevo firmware o recuperar un ASUS WL500 muerto?

Descomprime e instala el programa Restoration software en tu PC
Configura la tarjeta de red de tu PC con la IP 192.168.1.5, máscara 255.255.255.0, puerta de enlace 192.168.1.1
Conecta el router con el PC, cable ethernet.
Arranca el programa firmware restoration que está en el grupo programas Asus Utility/WL500GP...(en windows 7 debes arrancar con derechos de administrador)
Una vez dentro del programa en nombre del archivo carga el fichero wl500g-clear-nvram.trx
Desconecta el router, pulsa el botón de reset en la parte posterior y vuelve a conectar el router, espera a que el LED de Power parpadee y deja de pulsar el Reset del router. Espera 5 segundos.
Dale al Botón Activar en el programa. Se cargará un archivo. Espera a que el LED de Power del router se ilumine de nuevo y quede fijo.
Desconecta el router, pulsa el botón de reset en la parte posterior y vuelve a conectar el router, espera a que el LED de Power parpadee y deja de pulsar el Reset del router. Espera 5 segundos.
Con el mismo programa anterior carga el fichero wl500g-recover.trx, pulsa Activar.
Dale al Botón Activar en el programa. Se cargará un archivo. Pasados unos 3 minutos desconecta el router, pulsa el botón de reset en la parte posterior y vuelve a conectar el router, espera a que el LED de Power parpadee y deja de pulsar el Reset del router. Espera 5 segundos.
Con el mismo programa anterior carga el fichero del último firmware para este router (puedes usar cualquier firmware de los disponibles, Tomato, DD-WRT. Recuerda que debes cargar el fichero con extensión .trx, pulsa Activar.
Espera unos 3 minutos hasta que la luz de Power se ilumine de nuevo. Ya puedes salir del programa y con el navegador de Internet entrar en la web de configuración del router.

Usuario: Con firmware dd-wrt= root, con firmware ASUS y Tomato= admin
Password: Con todos los firmwares = admin

Ya tienes tu router funcionando de nuevo.

Saludos


Enjoy!

Victek.02/02/2011



