$Id: INTERFACE,v 1.1.4.1 2001/11/20 14:19:33 kai Exp $

Description of the Interface between Linklevel and Hardwarelevel
  of isdn4linux:


  The Communication between Linklevel (LL) and Hardwarelevel (HL)
  is based on the struct isdn_if (defined in isdnif.h).

  An HL-driver can register itself at LL by calling the function
  register_isdn() with a pointer to that struct. Prior to that, it has
  to preset some of the fields of isdn_if. The LL sets the rest of
  the fields. All further communication is done via callbacks using
  the function-pointers defined in isdn_if.

  Changes/Version numbering:

  During development of the ISDN subsystem, several changes have been
  made to the interface. Before it went into kernel, the package
  had a unique version number. The last version, distributed separately
  was 0.7.4. When the subsystem went into kernel, every functional unit
  got a separate version number. These numbers are shown at initialization,
  separated by slashes:

     c.c/t.t/n.n/p.p/a.a/v.v

  where

   c.c is the revision of the common code.
   t.t is the revision of the tty related code.
   n.n is the revision of the network related code.
   p.p is the revision of the ppp related code.
   a.a is the revision of the audio related code.
   v.v is the revision of the V.110 related code.

  Changes in this document are marked with '***CHANGEx' where x representing
  the version number. If that number starts with 0, it refers to the old,
  separately distributed package. If it starts with one of the letters
  above, it refers to the revision of the corresponding module. 
  ***CHANGEIx refers to the revision number of the isdnif.h  

1. Description of the fields of isdn_if:

  int channels;

    This field has to be set by the HL-driver to the number of channels
    supported prior to calling register_isdn(). Upon return of the call,
    the LL puts an id there, which has to be used by the HL-driver when
    invoking the other callbacks.

  int maxbufsize;

    ***CHANGE0.6: New since this version.

    Also to be preset by the HL-driver. With this value the HL-driver
    tells the LL the maximum size of a data-packet it will accept. 

  unsigned long features;

    To be preset by the HL-driver. Using this field, the HL-driver
    announces the features supported. At the moment this is limited to
    report the supported layer2 and layer3-protocols. For setting this
    field the constants ISDN_FEATURE..., declared in isdnif.h have to be
    used.

    ***CHANGE0.7.1: The line type (1TR6, EDSS1) has to be set.

  unsigned short hl_hdrlen;

    ***CHANGE0.7.4: New field.

    To be preset by the HL-driver, if it supports sk_buff's. The driver
    should put here the amount of additional space needed in sk_buff's for
    its internal purposes. Drivers not supporting sk_buff's should 
    initialize this field to 0.

  void (*rcvcallb_skb)(int, int, struct sk_buff *)

    ***CHANGE0.7.4: New field.

    This field will be set by LL. The HL-driver delivers received data-
    packets by calling this function. Upon calling, the HL-driver must
    already have its private data pulled off the head of the sk_buff.

    Parameter:
      int              driver-Id
      int              Channel-number locally to the driver. (starting with 0)
      struct sk_buff * Pointer to sk_buff, containing received data.

  int (*statcallb)(isdn_ctrl*);

    This field will be set by LL. This function has to be called by the
    HL-driver for signaling status-changes or other events to the LL.

    Parameter:
      isdn_ctrl*

      The struct isdn_ctrl also defined in isdn_if. The exact meanings of its
      fields are described together with the descriptions of the possible
      events. Here is only a short description of the fields:

        driver  = driver Id.
        command = event-type. (one of the constants ISDN_STAT_...)
        arg     = depends on event-type.
        num     = depends on event-type.

    Returnvalue:
      0 on success, else -1

  int (*command)(isdn_ctrl*);

    This field has to be preset by the HL-driver. It points to a function,
    to be called by LL to perform functions like dialing, B-channel
    setup, etc. The exact meaning of the parameters is described with the
    descriptions of the possible commands.

    Parameter:
      isdn_ctrl*
        driver  = driver-Id
        command = command to perform. (one of the constants ISDN_CMD_...)
        arg     = depends on command.
        num     = depends on command.
    
    Returnvalue:
      >=0 on success, else error-code (-ENODEV etc.)

  int (*writebuf_skb)(int, int, int, struct sk_buff *)

    ***CHANGE0.7.4: New field.
    ***CHANGEI.1.21: New field.

    This field has to be preset by the HL-driver. The given function will
    be called by the LL for delivering data to be send via B-Channel.

 
    Parameter:
      int              driver-Id ***CHANGE0.7.4: New parameter.
      int              channel-number locally to the HL-driver. (starts with 0)
      int	       ack ***ChangeI1.21: New parameter
		       If this is !0, the driver has to signal the delivery
		       by sending an ISDN_STAT_BSENT. If this is 0, the driver
		       MUST NOT send an ISDN_STAT_BSENT.
      struct sk_buff * Pointer to sk_buff containing data to be send via
                       B-channel.

    Returnvalue:
      Length of data accepted on success, else error-code (-EINVAL on
      oversized packets etc.)

  int (*writecmd)(u_char*, int, int, int, int);

    This field has to be preset by the HL-driver. The given function will be
    called to perform write-requests on /dev/isdnctrl (i.e. sending commands
    to the card) The data-format is hardware-specific. This function is
    intended for debugging only. It is not necessary for normal operation
    and never will be called by the tty-emulation- or network-code. If
    this function is not supported, the driver has to set NULL here.

    Parameter:
      u_char* pointer to data.
      int     length of data.
      int     flag: 0 = call from within kernel-space. (HL-driver must use
                        memcpy, may NOT use schedule())
                    1 = call from user-space. (HL-driver must use
                        memcpy_fromfs, use of schedule() allowed)
      int     driver-Id.
      int     channel-number locally to the HL-driver. (starts with 0)

***CHANGEI1.14: The driver-Id and channel-number are new since this revision.

    Returnvalue:
      Length of data accepted on success, else error-code (-EINVAL etc.)

  int (*readstat)(u_char*, int, int, int, int);

    This field has to be preset by the HL-driver. The given function will be
    called to perform read-requests on /dev/isdnctrl (i.e. reading replies
    from the card) The data-format is hardware-specific. This function is
    intended for debugging only. It is not necessary for normal operation
    and never will be called by the tty-emulation- or network-code. If
    this function is not supported, the driver has to set NULL here.

    Parameter:
      u_char* pointer to data.
      int     length of data.
      int     flag: 0 = call from within kernel-space. (HL-driver must use
                        memcpy, may NOT use schedule())
                    1 = call from user-space. (HL-driver must use
                        memcpy_fromfs, use of schedule() allowed)
      int     driver-Id.
      int     channel-number locally to the HL-driver. (starts with 0)

***CHANGEI1.14: The driver-Id and channel-number are new since this revision.

    Returnvalue:
      Length of data on success, else error-code (-EINVAL etc.)

  char id[20];
       ***CHANGE0.7: New since this version.

   This string has to be preset by the HL-driver. Its purpose is for
   identification of the driver by the user. Eg.: it is shown in the
   status-info of /dev/isdninfo. Furthermore it is used as Id for binding
   net-interfaces to a specific channel. If a string of length zero is
   given, upon return, isdn4linux will replace it by a generic name. (line0,
   line1 etc.) It is recommended to make this string configurable during
   module-load-time. (copy a global variable to this string.) For doing that,
   modules 1.2.8 or newer are necessary.

2. Description of the commands, a HL-driver has to support:

   All commands will be performed by calling the function command() described
   above from within the LL. The field command of the struct-parameter will
   contain the desired command, the field driver is always set to the
   appropriate driver-Id.

   Until now, the following commands are defined:

***CHANGEI1.34: The parameter "num" has been replaced by a union "parm" containing
                the old "num" and a new setup_type struct used for ISDN_CMD_DIAL
                and ISDN_STAT_ICALL callback.

   ISDN_CMD_IOCTL:

     This command is intended for performing ioctl-calls for configuring
     hardware or similar purposes (setting port-addresses, loading firmware
     etc.) For this purpose, in the LL all ioctl-calls with an argument
     >= IIOCDRVCTL (0x100) will be handed transparently to this
     function after subtracting 0x100 and placing the result in arg.
     Example:
       If a userlevel-program calls ioctl(0x101,...) the function gets
       called with the field command set to 1.

     Parameter:
       driver   = driver-Id.
       command  = ISDN_CMD_IOCTL
       arg      = Original ioctl-cmd - IIOCDRVCTL
       parm.num = first bytes filled with (unsigned long)arg
   
     Returnvalue:
       Depending on driver.

  
  ISDN_CMD_DIAL:

    This command is used to tell the HL-driver it should dial a given
    number.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_DIAL
      arg         = channel-number locally to the driver. (starting with 0)
      
      parm.setup.phone  = An ASCII-String containing the number to dial.
      parm.setup.eazmsn = An ASCII-Sting containing the own EAZ or MSN.
      parm.setup.si1    = The Service-Indicator.
      parm.setup.si2    = Additional Service-Indicator.

                    If the Line has been designed as SPV (a special german
                    feature, meaning semi-leased-line) the phone has to
                    start with an "S".
      ***CHANGE0.6: In previous versions the EAZ has been given in the
                    highbyte of arg.
    ***CHANGE0.7.1: New since this version: ServiceIndicator and AddInfo.

  ISDN_CMD_ACCEPTD:

    With this command, the HL-driver is told to accept a D-Channel-setup.
    (Response to an incoming call)

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_ACCEPTD
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_CMD_ACCEPTB:

    With this command, the HL-driver is told to perform a B-Channel-setup.
    (after establishing D-Channel-Connection)

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_ACCEPTB
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_CMD_HANGUP:

    With this command, the HL-driver is told to hangup (B-Channel if
    established first, then D-Channel). This command is also used for
    actively rejecting an incoming call.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_HANGUP
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_CMD_CLREAZ:

    With this command, the HL-driver is told not to signal incoming
    calls to the LL.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_CLREAZ
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_CMD_SETEAZ:

    With this command, the HL-driver is told to signal incoming calls for
    the given EAZs/MSNs to the LL.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_SETEAZ
      arg         = channel-number locally to the driver. (starting with 0)
      parm.num    = ASCII-String, containing the desired EAZ's/MSN's
                    (comma-separated). If an empty String is given, the
                    HL-driver should respond to ALL incoming calls,
                    regardless of the destination-address.
      ***CHANGE0.6: New since this version the "empty-string"-feature.

  ISDN_CMD_GETEAZ: (currently unused)

    With this command, the HL-driver is told to report the current setting
    given with ISDN_CMD_SETEAZ.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_GETEAZ
      arg         = channel-number locally to the driver. (starting with 0)
      parm.num    = ASCII-String, containing the current EAZ's/MSN's

  ISDN_CMD_SETSIL: (currently unused)

    With this command, the HL-driver is told to signal only incoming
    calls with the given Service-Indicators.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_SETSIL
      arg         = channel-number locally to the driver. (starting with 0)
      parm.num    = ASCII-String, containing the desired Service-Indicators.

  ISDN_CMD_GETSIL: (currently unused)

    With this command, the HL-driver is told to return the current
    Service-Indicators it will respond to.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_SETSIL
      arg         = channel-number locally to the driver. (starting with 0)
      parm.num    = ASCII-String, containing the current Service-Indicators.

  ISDN_CMD_SETL2:

    With this command, the HL-driver is told to select the given Layer-2-
    protocol. This command is issued by the LL prior to ISDN_CMD_DIAL or
    ISDN_CMD_ACCEPTD.


    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_SETL2
      arg         = channel-number locally to the driver. (starting with 0)
                    logical or'ed with (protocol-Id << 8)
                    protocol-Id is one of the constants ISDN_PROTO_L2...
      parm        = unused.

  ISDN_CMD_GETL2: (currently unused)

    With this command, the HL-driver is told to return the current
    setting of the Layer-2-protocol.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_GETL2
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.
    Returnvalue:
      current protocol-Id (one of the constants ISDN_L2_PROTO)

  ISDN_CMD_SETL3:

    With this command, the HL-driver is told to select the given Layer-3-
    protocol. This command is issued by the LL prior to ISDN_CMD_DIAL or
    ISDN_CMD_ACCEPTD.


    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_SETL3
      arg         = channel-number locally to the driver. (starting with 0)
                    logical or'ed with (protocol-Id << 8)
                    protocol-Id is one of the constants ISDN_PROTO_L3...
      parm.fax    = Pointer to T30_s fax struct. (fax usage only)

  ISDN_CMD_GETL2: (currently unused)

    With this command, the HL-driver is told to return the current
    setting of the Layer-3-protocol.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_GETL3
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.
    Returnvalue:
      current protocol-Id (one of the constants ISDN_L3_PROTO)

  ISDN_CMD_LOCK:

    With this command the HL-driver is told, that it will be used by the
    LL and therefore may not be unloaded. The HL-driver should use
    MOD_INC_USE_COUNT to tell that to the kernel.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_LOCK
      arg         = unused.
      parm        = unused.

  ISDN_CMD_UNLOCK:

    With this command the HL-driver is told, that it is no more used by the
    LL and therefore may be unloaded. The HL-driver should use
    DEC_INC_USE_COUNT to tell that to the kernel.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_UNLOCK
      arg         = unused.
      parm        = unused.

  ISDN_CMD_PROCEED: 

    With this command, the HL-driver is told to proceed with a incoming call.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_PROCEED
      arg         = channel-number locally to the driver. (starting with 0)
      setup.eazmsn= empty string or string send as uus1 in DSS1 with 
                    PROCEED message

  ISDN_CMD_ALERT: 

    With this command, the HL-driver is told to alert a proceeding call.

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_ALERT
      arg         = channel-number locally to the driver. (starting with 0)
      setup.eazmsn= empty string or string send as uus1 in DSS1 with 
                    ALERT message

  ISDN_CMD_REDIR: 

    With this command, the HL-driver is told to redirect a call in proceeding
    or alerting state.  

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_REDIR
      arg         = channel-number locally to the driver. (starting with 0)
      setup.eazmsn= empty string or string send as uus1 in DSS1 protocol
      setup.screen= screening indicator
      setup.phone = redirected to party number

  ISDN_CMD_PROT_IO:

    With this call, the LL-driver invokes protocol specific features through
    the LL.
    The call is not implicitely bound to a connection.

    Parameter:
      driver      = driver-Id
      command     = ISDN_CMD_PROT_IO
      arg         = The lower 8 Bits define the addressed protocol as defined
                    in ISDN_PTYPE..., the upper bits are used to differentiate
                    the protocol specific CMD.  
      
      para        = protocol and function specific. See isdnif.h for detail.


  ISDN_CMD_FAXCMD:

    With this command the HL-driver receives a fax sub-command.
    For details refer to INTERFACE.fax

    Parameter:
      driver      = driver-Id.
      command     = ISDN_CMD_FAXCMD
      arg         = channel-number locally to the driver. (starting with 0)
      parm        = unused.


3. Description of the events to be signaled by the HL-driver to the LL.

  All status-changes are signaled via calling the previously described
  function statcallb(). The field command of the struct isdn_cmd has
  to be set by the HL-driver with the appropriate Status-Id (event-number).
  The field arg has to be set to the channel-number (locally to the driver,
  starting with 0) to which this event applies. (Exception: STAVAIL-event)

  Until now, the following Status-Ids are defined:

  ISDN_STAT_AVAIL:

    With this call, the HL-driver signals the availability of new data
    for readstat(). Used only for debugging-purposes, see description
    of readstat().

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_STAVAIL
      arg         = length of available data.
      parm        = unused.

  ISDN_STAT_ICALL:
  ISDN_STAT_ICALLW:

    With this call, the HL-driver signals an incoming call to the LL.
    If ICALLW is signalled the incoming call is a waiting call without
    a available B-chan.

    Parameter:
      driver            = driver-Id
      command           = ISDN_STAT_ICALL
      arg               = channel-number, locally to the driver. (starting with 0)
      para.setup.phone  = Callernumber.
      para.setup.eazmsn = CalledNumber.
      para.setup.si1    = Service Indicator.
      para.setup.si2    = Additional Service Indicator.
      para.setup.plan   = octet 3 from Calling party number Information Element.
      para.setup.screen = octet 3a from Calling party number Information Element.

    Return:
      0           = No device matching this call.
      1           = At least one device matching this call (RING on ttyI).
                    HL-driver may send ALERTING on the D-channel in this case.
      2           = Call will be rejected.
      3           = Incoming called party number is currently incomplete.
                    Additional digits are required. 
                    Used for signalling with PtP connections.
      4	          = Call will be held in a proceeding state 
                    (HL driver sends PROCEEDING)
                    Used when a user space prog needs time to interpret a call
		    para.setup.eazmsn may be filled with an uus1 message of
		    30 octets maximum. Empty string if no uus. 
      5           = Call will be actively deflected to another party
                    Only available in DSS1/EURO protocol
		    para.setup.phone must be set to destination party number
		    para.setup.eazmsn may be filled with an uus1 message of
		    30 octets maximum. Empty string if no uus. 
      -1          = An error happened. (Invalid parameters for example.)
  The keypad support now is included in the dial command.	        


  ISDN_STAT_RUN:

    With this call, the HL-driver signals availability of the ISDN-card.
    (after initializing, loading firmware)

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_RUN
      arg         = unused.
      parm        = unused.

  ISDN_STAT_STOP:

    With this call, the HL-driver signals unavailability of the ISDN-card.
    (before unloading, while resetting/reconfiguring the card)

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_STOP
      arg         = unused.
      parm        = unused.

  ISDN_STAT_DCONN:

   With this call, the HL-driver signals the successful establishment of
   a D-Channel-connection. (Response to ISDN_CMD_ACCEPTD or ISDN_CMD_DIAL)

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_DCONN
      arg         = channel-number, locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_STAT_BCONN:

   With this call, the HL-driver signals the successful establishment of
   a B-Channel-connection. (Response to ISDN_CMD_ACCEPTB or because the
   remote-station has initiated establishment)

   The HL driver should call this when the logical l2/l3 protocol 
   connection on top of the physical B-channel is established.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_BCONN
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.num    = ASCII-String, containing type of connection (for analog
		    modem only). This will be appended to the CONNECT message
		    e.g. 14400/V.32bis

  ISDN_STAT_DHUP:

   With this call, the HL-driver signals the shutdown of a
   D-Channel-connection. This could be a response to a prior ISDN_CMD_HANGUP,
   or caused by a remote-hangup or if the remote-station has actively
   rejected a call.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_DHUP
      arg         = channel-number, locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_STAT_BHUP:

   With this call, the HL-driver signals the shutdown of a
   B-Channel-connection. This could be a response to a prior ISDN_CMD_HANGUP,
   or caused by a remote-hangup.

   The HL driver should call this as soon as the logical l2/l3 protocol 
   connection on top of the physical B-channel is released.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_BHUP
      arg         = channel-number, locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_STAT_CINF:

   With this call, the HL-driver delivers charge-unit information to the
   LL.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_CINF
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.num    = ASCII string containing charge-units (digits only).

  ISDN_STAT_LOAD: (currently unused)

  ISDN_STAT_UNLOAD:

   With this call, the HL-driver signals that it will be unloaded now. This
   tells the LL to release all corresponding data-structures.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_UNLOAD
      arg         = unused.
      parm        = unused.

  ISDN_STAT_BSENT:

    With this call the HL-driver signals the delivery of a data-packet.
    This callback is used by the network-interfaces only, tty-Emulation
    does not need this call.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_BSENT
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.length = ***CHANGEI.1.21: New field.
		    the driver has to set this to the original length
		    of the skb at the time of receiving it from the linklevel.

  ISDN_STAT_NODCH:

    With this call, the driver has to respond to a prior ISDN_CMD_DIAL, if
    no D-Channel is available.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_NODCH
      arg         = channel-number, locally to the driver. (starting with 0)
      parm        = unused.

  ISDN_STAT_ADDCH: 

    This call is for HL-drivers, which are unable to check card-type
    or numbers of supported channels before they have loaded any firmware
    using ioctl. Those HL-driver simply set the channel-parameter to a
    minimum channel-number when registering, and later if they know
    the real amount, perform this call, allocating additional channels.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_ADDCH
      arg         = number of channels to be added.
      parm        = unused.

  ISDN_STAT_CAUSE:

    With this call, the HL-driver delivers CAUSE-messages to the LL.
    Currently the LL does not use this messages. Their contents is simply
    logged via kernel-messages. Therefore, currently the format of the
    messages is completely free. However they should be printable.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_NODCH
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.num    = ASCII string containing CAUSE-message.

  ISDN_STAT_DISPLAY:

    With this call, the HL-driver delivers DISPLAY-messages to the LL.
    Currently the LL does not use this messages. 

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_DISPLAY
      arg         = channel-number, locally to the driver. (starting with 0)
      para.display= string containing DISPLAY-message.

  ISDN_STAT_PROT:

    With this call, the HL-driver delivers protocol specific infos to the LL.
    The call is not implicitely bound to a connection.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_PROT
      arg         = The lower 8 Bits define the addressed protocol as defined
                    in ISDN_PTYPE..., the upper bits are used to differenciate
                    the protocol specific STAT.  
      
      para        = protocol and function specific. See isdnif.h for detail.

  ISDN_STAT_DISCH:

    With this call, the HL-driver signals the LL to disable or enable the
    use of supplied channel and driver.
    The call may be used to reduce the available number of B-channels after
    loading the driver. The LL has to ignore a disabled channel when searching
    for free channels. The HL driver itself never delivers STAT callbacks for
    disabled channels. 	    
    The LL returns a nonzero code if the operation was not successful or the
    selected channel is actually regarded as busy.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_DISCH
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.num[0] = 0 if channel shall be disabled, else enabled.

  ISDN_STAT_L1ERR:

    ***CHANGEI1.21 new status message.
    A signal can be sent to the linklevel if an Layer1-error results in
    packet-loss on receive or send. The field errcode of the cmd.parm
    union describes the error more precisely.

    Parameter:
      driver      = driver-Id
      command     = ISDN_STAT_L1ERR
      arg         = channel-number, locally to the driver. (starting with 0)
      parm.errcode= ISDN_STAT_L1ERR_SEND:     Packet lost while sending.
		    ISDN_STAT_L1ERR_RECV:     Packet lost while receiving.
  ISDN_STAT_FAXIND:

    With this call the HL-driver signals a fax sub-command to the LL.
    For details refer to INTERFACE.fax

    Parameter:
      driver      = driver-Id.
      command     = ISDN_STAT_FAXIND
      arg         = channel-number, locally to the driver. (starting with 0)
      parm        = unused.

